Experiment 6: Double-Slit Interference

Introduction:

Theory:

Experimental Method:

1. Done
2. Amplification adjusted for full scale reading.
3. Whilst rotating the Goniometer arm, the meter readings vary from minima to maxima – 5 maxima are located between 90 degrees and 270 degrees – this is likely due to constructive and destructive interference from the double slit.